Package: VICmodel
Type: Package
Title: The Variable Infiltration Capacity (VIC) Model
Version: 0.1.2
Date: 2018-11-08
Authors@R: c(person("Ruida", "Zhong", email = "zrd2017@163.com", role = c("aut", "cre")),
    person("Xiaohong", "Chen", email = "eescxh@mail.sysu.edu.cn", role = c("aut", "ctb")),
    person("Zhaoli", "Wang", email = "wangzhl@scut.edu.cn", role = c("aut", "ctb")),
    person("Chengguang", "Lai", email = "laichg@scut.edu.cn", role = c("aut", "ctb")),
    person("Joseph J", "Hamman", role = c("ctb"), comment = "Contributor and maintainer of VIC source code"),
    person("Keith", "Cherkauer", role = c("ctb"))
    )
Description: The Variable Infiltration Capacity (VIC) model is a macroscale
    hydrologic model that solves full water and energy balances, originally
    developed by Xu Liang at the University of Washington (UW).
    The version of VIC source code used is of 5.0.1 on <https://github.com/UW-Hydro/VIC/>,
    see Hamman et al. (2018).
    Development and maintenance of the current official version
    of the VIC model at present is led by the UW Hydro (Computational Hydrology
    group) in the Department of Civil and Environmental Engineering at UW. VIC is
    a research model and in its various forms it has been applied to most of the
    major river basins around the world, as well as globally. If you make use of
    this model, please acknowledge the appropriate references listed in the help
    page of this package or on the references page
    <http://vic.readthedocs.io/en/master/Documentation/References/>
    of the VIC official documentation website.
    These should include Liang et al. (1994) plus any references relevant to the
    features you are using Reference: Liang, X., D. P. Lettenmaier, E. F. Wood, and
    S. J. Burges (1994), A simple hydrologically based model of land surface water
    and energy fluxes for general circulation models, J. Geophys. Res., 99(D7),
    14415-14428, <doi:10.1029/94JD00483>. Hamman et al. (2018) about VIC 5.0.1 also can
    be considered:
    Hamman, J. J., Nijssen, B., Bohn, T. J., Gergel, D. R., and Mao, Y. (2018), The
    Variable Infiltration Capacity model version 5 (VIC-5): infrastructure improvements
    for new applications and reproducibility, Geosci. Model Dev., 11, 3481-3496, 
    <doi:10.5194/gmd-11-3481-2018>.
License: GPL-3
Copyright: file inst/COPYRIGHTS
URL: https://github.com/Sibada/VICmodel
Encoding: UTF-8
LazyData: true
Depends: R (>= 3.0.0)
Imports: stats, utils, Rcpp (>= 0.12.0), foreach
Suggests: doParallel
LinkingTo: Rcpp
RoxygenNote: 5.0.1
NeedsCompilation: yes
Packaged: 2018-11-08 02:04:20 UTC; vicerTi
Author: Ruida Zhong [aut, cre],
  Xiaohong Chen [aut, ctb],
  Zhaoli Wang [aut, ctb],
  Chengguang Lai [aut, ctb],
  Joseph J Hamman [ctb] (Contributor and maintainer of VIC source code),
  Keith Cherkauer [ctb]
Maintainer: Ruida Zhong <zrd2017@163.com>
Repository: CRAN
Date/Publication: 2018-11-10 07:20:03 UTC
Built: R 3.4.4; x86_64-w64-mingw32; 2019-04-25 19:57:45 UTC; windows
Archs: i386, x64
