# Suite of GR Hydrological Models for Precipitation-Runoff Modelling

## Documentation for package ‘airGR’ version 1.4.3.65

- DESCRIPTION file.
- User guides, package vignettes and other documentation.

## Help Pages

airGR | Suite of GR Hydrological Models for Precipitation-Runoff Modelling
BasinInfo | Data sample: characteristics of a different catchments
BasinObs | Data sample: time series of observations of different catchments
Calibration | Calibration algorithm that optimises the error criterion selected as objective function using the provided functions
Calibration_Michel | Calibration algorithm that optimises the error criterion selected as objective function using the Irstea procedure described by C. Michel
CreateCalibOptions | Creation of the CalibOptions object required but the Calibration functions
CreateIniStates | Creation of the IniStates object possibly required by the CreateRunOptions functions
CreateInputsCrit | Creation of the InputsCrit object required to the ErrorCrit functions
CreateInputsModel | Creation of the InputsModel object required to the RunModel functions
CreateRunOptions | Creation of the RunOptions object required to the RunModel functions
DataAltiExtrapolation_Valery | Altitudinal extrapolation of precipitation and temperature series described by A. Valery
ErrorCrit | Error criterion using the provided function
ErrorCrit_KGE | Error criterion based on the KGE formula
ErrorCrit_KGE2 | Error criterion based on the KGE' formula
ErrorCrit_NSE | Error criterion based on the NSE formula
ErrorCrit_RMSE | Error criterion based on the RMSE
exampleSimPlot | Default preview of model outputs
Imax | Computation of the maximum capacity of the GR5H interception store
L0123001 | Data sample: time series of observations of different catchments
L0123002 | Data sample: time series of observations of different catchments
L0123003 | Data sample: time series of observations of different catchments
Param_Sets_GR4J | Generalist parameter sets for the GR4J model
PEdaily_Oudin | Computation of series of potential evapotranspiration at the daily or hourly time steps with Oudin's formula
PE_Oudin | Computation of series of potential evapotranspiration at the daily or hourly time steps with Oudin's formula
plot | Default preview of model outputs
plot.OutputsModel | Default preview of model outputs
RunModel | Run with the provided hydrological model function
RunModel_CemaNeige | Run with the CemaNeige snow module
RunModel_CemaNeigeGR4H | Run with the CemaNeigeGR4H hydrological model
RunModel_CemaNeigeGR4J | Run with the CemaNeigeGR4J hydrological model
RunModel_CemaNeigeGR5H | Run with the CemaNeigeGR5H hydrological model
RunModel_CemaNeigeGR5J | Run with the CemaNeigeGR5J hydrological model
RunModel_CemaNeigeGR6J | Run with the CemaNeigeGR6J hydrological model
RunModel_GR1A | Run with the GR1A hydrological model
RunModel_GR2M | Run with the GR2M hydrological model
RunModel_GR4H | Run with the GR4H hydrological model
RunModel_GR4J | Run with the GR4J hydrological model
RunModel_GR5H | Run with the GR5H hydrological model
RunModel_GR5J | Run with the GR5J hydrological model
RunModel_GR6J | Run with the GR6J hydrological model
SeriesAggreg | Conversion of time series to another time step (aggregation only)
simCNGR4J | Default preview of model outputs
simGR4J | Default preview of model outputs
TransfoParam | Transformation of the parameters using the provided function
TransfoParam_CemaNeige | Transformation of the parameters using the provided function
TransfoParam_CemaNeigeHyst | Transformation of the parameters using the provided function
TransfoParam_GR1A | Transformation of the parameters using the provided function
TransfoParam_GR2M | Transformation of the parameters using the provided function
TransfoParam_GR4H | Transformation of the parameters using the provided function
TransfoParam_GR4J | Transformation of the parameters using the provided function
TransfoParam_GR5H | Transformation of the parameters using the provided function
TransfoParam_GR5J | Transformation of the parameters using the provided function
TransfoParam_GR6J | Transformation of the parameters using the provided function
X0310010 | Data sample: time series of observations of different catchments