# Implementation of the Dynamic TOPMODEL Hydrological Model

## Documentation for package ‘dynatopmodel’ version 1.2.1

- DESCRIPTION file.
- Package NEWS.

## Help Pages

dynatopmodel-package | Implementation of the Dynamic TOPMODEL hydrological model.
aggregate_obs | Resample observation data at a new time interval
aggregate_xts | Resample observation data at a new time interval
approx.pe.ts | Create sinsuiodal time series of potential evapotranspiration input
brompton | Topographic and observation data for running Dynamic TOPMODEL.
build_chans | Construct a raster of channel locations from vector or topographic data
build_layers | Construct basic landscape layer data for Dynamic TOPMODEL run
build_routing_table | Generate a network routing table
dev.reset | Reset device parameters
discretise | Discrete a catchment into hydrological response units (HRUs)
disp_output | Display output of a Dynamic TOPMODEL run
dynatopmodel | Implementation of the Dynamic TOPMODEL hydrological model.
get.disp.par | Default list of parameters to control the graphical output during model simulation and via disp.output
get.run.par | get.run.par Initalise model run parameters. Note this function is maintained for backward compatibility only
Mode | Mode - modal value
new_guid | Get one or more GUIDs
NSE | Nash Sutcliffe Efficiency of a model's output against observations
run.dtm | Run Dynamic TOPMODEL against hydrometric data and a catchment discretisation
time_at_peak | Time of maximum observation
time_to_peak | Time between the peak rainfall and the peak discharge
upslope.area | Upslope contributing area and wetness index calculation