# Environmental Seismology Toolbox

## Documentation for package ‘eseis’ version 0.4.0

- DESCRIPTION file.
- Package NEWS.

## Help Pages

eseis-package | eseis: Environmental Seismology Toolbox
aux_fixmseed | Fix corrupt miniseed files
aux_getevent | Load seismic data of a user-defined event
aux_getFDSNdata | Download seismic data from FDSN data base
aux_getFDSNstation | Query FDSN data base for stations
aux_getIRISdata | Download seismic data from IRIS data base
aux_getIRISstation | Query IRIS data base for stations
aux_gettemperature | Extract temperature data from cube files.
aux_hvanalysis | Perform H-V-spectral ratio analysis of a seismic data set
aux_initiateeseis | Initiate an eseis object
aux_organisecentaurfiles | Reorganise seismic files recorded by Nanometrics Centaur loggers
aux_organisecubefiles | Convert Omnirecs/Digos Datacube files to mseed or sac files and organise in directory structure.
aux_psdpanels | Generate spectrogram panels for a seismic network
aux_psdsummary | Generate spectrograms for seismic stations at different time periods
aux_stationinfofile | Create station info file from cube files.
earthquake | Seismic traces of a small earthquake
eseis | eseis: Environmental Seismology Toolbox
list_logger | List library with data logger information.
list_sacparameters | List all header parameters of a sac file.
list_sensor | List sensor library.
model_turbulence | Model the seismic spectrum due to hydraulic turbulence
plot_components | Plot three seismic components against each other
plot_ppsd | Plot a probabilistic power spectral density estimate (PPSD)
plot_signal | Plot a seismic signal
plot_spectrogram | Plot spectrograms (power spectral density estimates)
plot_spectrum | Plot a spectrum of a seismic signal
read_mseed | Read mseed files.
read_sac | Read sac files.
rockfall | Seismic trace of a rockfall event.
rockfall_eseis | Seismic trace of a rockfall event.
rockfall_t | Seismic trace of a rockfall event.
rockfall_z | Seismic trace of a rockfall event.
s | Seismic traces of a small earthquake
signal_aggregate | Aggregate a signal vector
signal_clip | Clip signal based on time vector.
signal_deconvolve | Deconvolve a signal vector.
signal_demean | Remove mean of signal vector.
signal_detrend | Detrend a signal vector.
signal_envelope | Calculate signal envelope.
signal_filter | Filter a seismic signal in the time domain
signal_hilbert | Calculate Hilbert transform.
signal_hvratio | Calculate h-v-ratio of seismic components
signal_integrate | Integrate a seismic signal
signal_motion | Calculate particle motion parameters
signal_pad | Pad signal with zeros.
signal_rotate | Rotate signal vectors using a 3-D rotation matrix.
signal_snr | Calculate signal-to-noise-ratio.
signal_spectrogram | Calculate spectrograms (power spectral density estimates) from time series.
signal_spectrum | Calculate the spectrum of a time series
signal_stalta | Calculate stal-lta-ratio.
signal_sum | Calculate signal vector sum.
signal_taper | Taper a signal vector.
spatial_clip | Clip values of spatial data.
spatial_convert | Convert coordinates between reference systems
spatial_distance | Calculate topography-corrected distances for seismic waves.
spatial_migrate | Migrate signals of a seismic event through a grid of locations.
t | Seismic traces of a small earthquake
time_aggregate | Aggregate a time series
time_clip | Clip time vector.
time_convert | Convert Julian Day to Date and vice versa
write_report | Create a HTML report for (RLum) objects
write_sac | Write seismic traces as sac file to disk.