# Handling Multiplatform Satellite Images

## Documentation for package ‘RGISTools’ version 1.0.2

- DESCRIPTION file.

## Help Pages

RGISTools-package | 'RGISTools': Handling Multiplatform Satellite Images
ex.dem.navarre | A Digital Elevation Model (DEM) of the region of Navarre (Spain)
ex.navarre | A polygon with the border of Navarre (Spain)
ex.ndvi.navarre | A time series of NDVI of Navarre (Spain)
genCompositions | Create image compositions from a time series of satellite images
genFilterStack | Subset a RasterStack given a range of dates
genGetDates | Return the capturing date from the name of a raster layer
genMosaicList | Mosaic a list of raster images
genPlotGIS | Plot satellite images with a GIS format
genSaveTSRData | Saves a time series of images as an RData
genSmoothingCovIMA | Fill data gaps and smooth outliers in a time series of satellite images using covariates
genSmoothingIMA | Fill data gaps and smooth outliers in a time series of satellite images
getRGISToolsOpt | Get the default value of an RGISTools option
ls7FolderToVar | Compute a remote sensing index from a time series of Landsat-7 images
ls7LoadMetadata | Load or update the Landsat-7 metadata file
ls7Search | Search Landsat-7 images
ls8FolderToVar | Compute a remote sensing index from a time series of Landsat-8 images
ls8LoadMetadata | Load or update the Landsat-8 metadata file
ls8Search | Search Landsat-8 images
lsCloudMask | Create cloud masks for Landsat images
lsDownload | Download Landsat-7 or Landsat-8 images from a search list
lsDownSearch | Search and download Landsat-7 or Landsat-8 images
lsEspaDownloadOrders | Downloads the images that have been pre-processed by ESPA
lsEspaGetOrderImages | Gets a first response from ESPA regarding a recent request
lsEspaOrderImages | Make a request to ESPA for pre-processing Landsat images
lsEspaUpdateOrders | Updates the status of a request made to ESPA
lsGetDates | Return the capturing dates of Landsat-7 or Landsat-8 images
lsGetPathRow | Return the pathrow of a tile of Landsat-7 or Landsat-8 images
lsMosaic | Mosaic a set of Landsat-7 or Landsat-8 images
lsPreview | Preview Landsat-7 or Landsat-8 satellite images
lsRemoveMetadata | Remove the Landsat-7 or Lansat-8 metadata from the environment
lsSearch | Search Landsat 7-8 images using EarthExplorer API
lsUpdateEEDataSets | Update EarthExplorer dataset names
modCloudMask | Create cloud masks for MODIS images
modDownload | Download MODIS images from a search list
modDownSearch | Search and download MODIS images
modExtractHDF | Convert an HDF file into a set of GTiff files
modFolderToVar | Compute a remote sensing index from a time series of MODIS multispectral images
modGetDates | Return the capturing dates of MODIS images
modGetPathRow | Return the pathrow of a tile of MODIS images
modMosaic | Mosaic a set of MODIS images
modPreview | Preview MODIS satellite images
modSearch | Search MODIS images
senCloudMask | Create cloud masks for Sentinel-2 images
senDownload | Download Sentinel images from a search list
senDownSearch | Search and download Sentinel images
senFolderToVar | Compute a remote sensing index from a time series of Sentinel-2 images
senGetDates | Return the capturing dates of Sentinel-2 images
senGetOrbit | Return the relative orbit of the Sentinel-2 satellite
senGetTile | Return the pathrow of a tile from Sentinel-2 images
senMosaic | Mosaic a set of Sentinel-2 images
senPreview | Preview Sentinel-2 satellite images
senSearch | Search Sentinel images
setRGISToolsOpt | Change the default value of an RGISTools option
showRGISToolsOpt | Print the name of all RGISTools configuration variables
varEVI | Calculate the enhanced vegetation index (EVI)
varMSAVI2 | Calculate the modified soil-adjusted vegetation index (MSAVI2)
varNBR | Calculate the normalized burn ratio (NBR)
varNBR2 | Calculate the normalized burn ratio 2 (NBR2)
varNDMI | Calculate the normalized difference moisture (water) index (NDMI)
varNDVI | Calculate the normalized difference vegetation index (NDVI)
varNDWI | Calculates the normalized difference water index (NDWI)
varRGB | Generate an RGB image from 3 spectral bands
varSAVI | Calculates the soil-adjusted vegetation index (SAVI)