Package: SunsVoc
Type: Package
Title: Constructing Suns-Voc from Outdoor Time-Series I-V Curves
Version: 0.1.0
Authors@R: c(person("Menghong", "Wang", email="mxw477@case.edu",
                    role=c("aut"), comment = c(ORCID = "0000-0001-7349-699X")),
            person("Tyler J.", "Burleyson", email="tjb152@case.edu",
                    role=c("aut","cre"), comment = c(ORCID = "0000-0002-6356-5354")),
            person("Jiqi", "Liu", email="jxl1763@case.edu",
                    role=c("aut"), comment = c(ORCID = "0000-0003-2016-4160")),
            person("Alan J.", "Curran", email="ajc269@case.edu",
                    role=c("aut"), comment = c(ORCID = "0000-0002-4505-8359")),
            person("Eric J.", "Schneller", email="eschneller@knights.ucf.edu",
                    role=c("aut"), comment = c(ORCID = "0000-0002-2104-0066")),
            person("Kristopher O.", "Davis", email="Kristopher.Davis@ucf.edu",
                    role=c("aut"), comment = c(ORCID = "0000-0002-5772-6254")),
            person("Jennifer L.", "Braid", email="jlb269@case.edu",
                    role=c("aut"), comment = c(ORCID = "0000-0002-0677-7756")),
            person("Roger H.", "French", email="rxf131@case.edu",
                    role=c("aut", "cph"), comment = c(ORCID = "0000-0002-6162-0532")))
Maintainer: Tyler J. Burleyson <tjb152@case.edu>
Description: 
    Suns-Voc (or Isc-Voc) curves can provide the current-voltage (I-V) characteristics of the
    diode of photovoltaic cells without the effect of series resistance.
    Here, Suns-Voc curves can be constructed with outdoor time-series I-V
    curves [1,2,3] of full-size photovoltaic (PV) modules instead of having to be measured in the lab.
    Time series of four different power loss modes can be calculated based on obtained Suns-Voc curves.
    This material is based upon work supported by the U.S. Department of
    Energy's Office of Energy Efficiency and Renewable Energy (EERE) under
    Solar Energy Technologies Office (SETO) Agreement Number DE-EE0008172. 
    Jennifer L. Braid is supported by the U.S. Department of Energy (DOE) Office of 
    Energy Efficiency and Renewable Energy administered by the Oak Ridge 
    Institute for Science and Education (ORISE) for the DOE. 
    ORISE is managed by Oak Ridge Associated Universities (ORAU) under DOE
    contract number DE-SC0014664. 
    [1] Wang, M. et al, 2018. 
    <doi:10.1109/PVSC.2018.8547772>. 
    [2] Walters et al, 2018
    <doi:10.1109/PVSC.2018.8548187>. 
    [3] Guo, S. et al, 2016. 
    <doi:10.1117/12.2236939>. 
License: BSD_3_clause + file LICENSE
Encoding: UTF-8
LazyData: true
RoxygenNote: 7.1.0
Depends: R (>= 3.5.0)
Imports: ddiv, magrittr, stringr, dplyr, purrr, data.table, rlang
Suggests: testthat (>= 2.1.0), knitr, rmarkdown, ggplot2
VignetteBuilder: knitr
NeedsCompilation: no
Packaged: 2020-06-26 15:53:26 UTC; tylerb
Author: Menghong Wang [aut] (<https://orcid.org/0000-0001-7349-699X>),
  Tyler J. Burleyson [aut, cre] (<https://orcid.org/0000-0002-6356-5354>),
  Jiqi Liu [aut] (<https://orcid.org/0000-0003-2016-4160>),
  Alan J. Curran [aut] (<https://orcid.org/0000-0002-4505-8359>),
  Eric J. Schneller [aut] (<https://orcid.org/0000-0002-2104-0066>),
  Kristopher O. Davis [aut] (<https://orcid.org/0000-0002-5772-6254>),
  Jennifer L. Braid [aut] (<https://orcid.org/0000-0002-0677-7756>),
  Roger H. French [aut, cph] (<https://orcid.org/0000-0002-6162-0532>)
Repository: CRAN
Date/Publication: 2020-06-29 10:40:03 UTC
Built: R 4.0.2; ; 2020-08-02 08:14:49 UTC; windows
